{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":5,"n_cols":7,"rows_kept":5,"merged":[[0,0,0,6],[4,0,4,6]],"flags":["formulas_cached_only"]}
["山东新闻大厦新闻餐厅桌椅采购清单"]
["序号","产品","规格","数量","参考图片","技术参数","备注"]
[1,"餐桌","1200*800*760",80,null,"餐桌桌面需采用刨花板或更优材质，具体要求如下：\n1.板材：优质环保E1级或更高刨花板。耐磨转数≥4000转，密度≥650kg/m³，甲醛释放量≤E1级（GB 18580-2017），提供CMA认证检测报告；\n2.面材：防潮MDF+防火板贴面；\n3.封边：优质PVC同色封边,封边工艺完整无缺损，边缘倒圆角R≥5mm；\n4.桌面整体厚度≥25mm；\n5.钢架：国标201不锈钢管。","1.桌腿类似样图中圆盘柱式或工字型钢架式，确保四角、四边不堵，不挡腿；\n2.桌椅板材颜色一致"]
[3,"餐椅","椅面高450-430（可调节误差±5mm）\n椅面最宽处≥415，确保成年人舒适就坐；\n顶部距地面850±10mm，提供腰部支撑区域高度≥150mm\n与桌面高度协调，符合人体工学设计。",320,null,"1.座面及椅背采用15mm环保多层板（E1级），层数≥11层，高压贴面处理；\n2.国标201不锈钢椅架管材厚度≥1.2mm，焊接点满焊打磨，底部配防滑脚垫；\n3.性能：静态承重≥150kg，通过5万次疲劳测试，防潮吸水率≤8%。","桌椅板材颜色一致"]
["注：图片仅供参考"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}